**DTF (DIRECT TO FILM)**

Direct-to-film (DTF) printing is a heat-transfer based print process whereby designs are printed onto a [transfer film](https://gjs.co/supplies/p4533/direct-to-film-dtf-matt-coating-film) using textile inks, which is then covered with a [thermo-adhesive powder](https://gjs.co/supplies/p4534/direct-to-film-dtf-thermo-adhesive-powder) and then transferred from the film to the garment using a heat press. Can be applied to a multitude of fabrics including polyester. The thermo-adhesive powder creates a white backing, so the colours stay vibrant, even on darker fabrics.

Thickness: 75 Micron.

Finish: Matt.

Available sizes: 600mm.

Length: 100m.

**FINISHING FILMS**

INDOOR LAMINATION

A pressure sensitive PVC film with a solvent-acrylic adhesive used for the protection of digital prints. Protect your prints from moisture and UV rays, as well as making them scratch resistant. Also helps to slow down the fading of the ink. These laminating films can also be used for short term outdoor applications.

Thickness: 80 Micron.

Finish: Matt, Gloss.

Available sizes: 1370mm, 1524mm.

Length: 50m.

OUTDOOR LAMINATION

A pressure sensitive PVC film with a solvent-acrylic adhesive and UV inhibitors used for the protection of digital prints. Protect your prints from moisture and UV rays, as well as making them scratch resistant. Also helps to slow down the fading of the ink. Suitable for indoor and longer term outdoor use.

Thickness: 80 Micron.

Finish: Matt, Gloss, Crystal Matt.

Available sizes: 1370mm, 1524mm, 1530mm.

Length: 50m.

DOUBLE-SIDED MOUNTING FILM

A clear polyester mounting film, coated on both sides with a permanent pressure sensitive acrylic adhesive, one of which is protected by a Kraft siliconized release liner and one side a film release liner. The perfect product for the mounting of graphics onto various substrates such as correx etc.

Thickness: 45 Micron.

Finish: N/A.

Available sizes: 1040mm, 1270mm.

Length: 33m.

OPTICALLY CLEAR DOUBLE-SIDED MOUNTING FILM

A 100% optically transparent polyester film. Both sides of the film have a high-viscosity solvent-acrylic adhesive that are protected by a clear film lining. Used for special applications that require full clarity, such as mounting a print to acrylic or glass.

Thickness: 25 Micron.

Finish: N/A.

Available sizes: 1300mm.

Length: 25m, 50m.